QGIS instructions for loading UK3D Cross-sections

Open a blank map, and set the Coordinate system as British National Grid (EPSG: 27700)

Load UK3D\_QGIS\_Version.gpkg into your map

Click View -> New 3D Map View

Click on the setting (spanner) icon in the 3D window and change the vertical scale to 10. Click Ok.

Right click on the Cross-sections layer in the table of contents and choose Properties. Select the 3D tab, and at the bottom of the dialog box click on Styles -> Load Style. Choose UK3D\_QGIS\_Styling\_ALL.qml. Click Load Style and all the geological unit names should be shown. Click Ok.

Your 3D map should now colour up with the correct BGS colours!